<@center><b><#selectbg_g>jolla-kernel ChangeLog</#></b>

<b><#selectbg_g>jollaman999 @xda developers</#></b>
<b><#selectbg_g>https://github.com/jollaman999</#></b>

<b><#selectbg_g>[bullhead_II-v22.1]</#></b></@>
== Kernel ==
- misc: fpc1020: Set fingerprintd priority to max when screen is off (by sultanxda)
- cpufreq: Introduce fingerprint boost driver (by frap129 origin codes by sultanxda)
- + Minor fixes for fingerprint boost driver

== AIO ==
- Updater: Check the error of executing su command (Fix force close when SU is not allowed for updater.)
- Updater: Cleanup unused usages
- Updater: Show toast messages for a long time
- Updater: Version up to v1.9

== Recovery ==
- Appiled jolla-kernel_bullhead_II-v22.1

<b><#selectbg_g>[bullhead_II-v22.0]</#></b>
== Kernel ==
- Appiled Android O DP2 patches
- f2fs: Add missed 'bio_put(bio)' in 'f2fs_submit_discard_endio()'
- nanohub: Applied lastest marlin patches and Android O DP2 patch from Google msm
- kernel: Only expose su when daemon is running (from LineageOS android_kernel_oneplus_msm8996)
- kernel: Fix potential refcount leak in su check (from LineageOS android_kernel_oneplus_msm8996)
- sdcardfs: Applied lastest android-3.10 patches from Google android-3.10
- net/packet: Fix overflow patches from Google android-3.10
- msm_thermal: Check high temp and decrease LITTLE's frequency to lower values
( When big core is turned off, LITTLE's decrease step will set to 2
by 'temp_count_max_little_with_big_off'.
 In some cases, when device is too hot, there is no way to decrease frequency.
 It needs to check high temp to get lower frequencies of LITTLE cores.)
- arm/arm64: Applies some complie related patches from Google android-3.10

== AIO ==
- Updater: Update libraries to O
- Updater: Main: Do not call 'getApplicationContext()' when not needed
- Updater: Fix SELinux denials and check root status
- Updater: Version up to v1.8
- A2DP Checker: Update libraries to O

== Recovery ==
- Appiled lastest omni TWRP patches
- Built with lastest LineageOS sources
- Appiled jolla-kernel_bullhead_II-v22.0

<b><#selectbg_g>[bullhead_II-v21.0]</#></b>
== Kernel ==
- Built with Linaro gcc-linaro-6.3.1-2017.05-rc1
- Applied timerfd, tty and net patches from Google android-3.10
- sdcardfs: Applied lastest android-3.10 patches from Google android-3.10
- f2fs: Appied linux-4.4.y stable branch patches from jaegeuk/f2fs-stable

== AIO ==
- f2fs-tools: Applied lastest dev branch patches from jaegeuk/f2fs-tools

== Recovery ==
- Built with lastest LineageOS sources
- Update TWRP to AOSP 7.1.2
- TWRP version up to 3.1.1
- Appiled jolla-kernel_bullhead_II-v21.0

<b><#selectbg_g>[bullhead_II-v20.0]</#></b>
== Kernel ==
- May!
- sdcardfs: Applied lastest android-3.10 patches from Google android-3.10
- ext2, ext4, mbcache patch from Google android-3.10

== AIO ==
- None

== Recovery ==
- Appiled jolla-kernel_bullhead_II-v20.0


<b><#selectbg_g>[Thanks to..]</#></b>
The Linux Kernel Archives : https://www.kernel.org/
LineageOS : https://github.com/LineageOS
Developers : jaegeuk, Tasssadar, savoca and all of commited in their sources & all of xda developers

<#selectbg_g>->></#> Thank You for choosing my jolla-kernel!! :)
